Specifications
08/15/2024

		Project
	From
	
		UNOX Natural Gas Double Stack 6 pan Combis specifications with Pre-Built option and extended warranty

ITEM 1 -COMBI OVEN, GAS  (2  REQ'D) 
UNOX USA Model XAVC-06FS-GPRM Dimensions: 33.13(h) x 33.88(w) x 38.06(d).  No Alternates Accepted.
 
ChefTop MIND.Maps™ Plus Combi Oven/Steam Oven is a gas countertop oven that combines heat, hot air flow and steam. (6) 18" x 26" full size sheet or (12) hotel size pan capacity, MIND.Maps™ technology, programmable menu, 2-11/16" shelf spacing, glass door, right-to-left door opening, stainless steel interior & exterior, WIFI/USB for data transfer to HACCP software, 1kW, 8 amps, 120v/60/1-ph, cETLus, NSF, ENERGY STAR® (cooking chamber built from 316L stainless steel) 
(For safety and reliability purposes, CHEFTOP MIND.Maps™ Gas ovens (Free Standing and Countertop Models) must be equipped with only UNOX brand casters with safety chains),Gas lines is not included with the oven and must be purchased separately. Ovens come standard with rack slides for sheet pans.
1 ea	Model INSTALL FORM End User Data & Installation Confirmation Form
1 ea	2 Year parts and 1 year labor warranty standard
2 ea	Model LL4-2 Long.Life 4 years warranty/10,000 working hours on parts and 2 years labor
1 ea	Model PREBUILT-2 Prebuilt, ready to connect stacked units (Required 2 Units).  UNOX combi’s are stacked at the factory and water filters are installed to the ovens.  This option is used when no purchasing the install from UNOX. 
1 ea	Start-Up option is intended for customers who purchase pre-built or install equipment on their own and in both cases make all electrical and mechanical connections prior to Start-Up visit. Start-Up includes travel within a 100-mile radius (200 miles round trip) of the UNOX approved technician (one trip). The service is the act of an authorized technician reviewing all electrical and mechanical connections for correctness in accordance with the manufacturers written specifications. The authorized technician will also power unit on for the first time, perform all calibrations, operational & functional tests.
1 ea	Model STARTUP-1 Start-Up 1st Unit
1 ea	Model STARTUP-2 Start-Up 2nd or more unit(s)
2 ea	Natural gas
1 ea	Model XAAQC-00E2-G Stacking Kit for ChefTop MIND.Maps™ Plus, includes installation kits and stacking parts for stacking two ovens, for gas ovens including floor stand (XWARC-00-EF-F) and casters (XUC012)
2 ea	Model UXGL-3448A Unox/Dormont Blue Hose™ Moveable Gas Connector Kit, 3/4" inside dia., 48" long, covered with stainless steel braid, coated with blue antimicrobial PVC, (1) SnapFast® QD, (1) full port valve, (2) 90° elbows, (1) Snap'N Go, coiled restraining cable with hardware, 180,000 BTU/hr minimum flow capacity, limited lifetime warranty
2 ea	It is the sole responsibility of the owner/operator/purchaser of this equipment to verify that the incoming water supply is comprehensively tested (Free Chlorine, Chloramine, TDS (Total Dissolved Solids), Silica, pH, TH (Total Hardness), Chlorides & Alkalinity) & if required, provide a means of water treatmeant that would meet the minimum requirements of the manufacturer's water quality standards as outlined on the product spec sheet. Non-compliance with these minimum standards will potentially damage this equipment and/or components & VOID the original equipment manufacturer's warranty
2 ea	Model UX170-52080A QT1+CR, QT Water Filter System, dual, (1) 10" CTO-Q10 cartridge & (1) 15" CTO-QCR cartridge, 20,000 gallon capacity, 2.5 gpm flow rate, reduces chlorine, taste & odor - 6,000 gallon capacity, 0.5 gpm, reduces chloramine, 0.5 micron particulate. *Standard Pentair® Limited Warranty*
2 ea	Model DB1018A0 UNOX Detergent & Rinse Eco, (10) 1 liter tanks, double concentrate, phosphate free, cleaning chemicals for Rotor. Klean™ (There is a hazardous shipping charge for detergents)
12 ea	Model GRP560 CHROMO.GRID, 18"x26", stainless steel

While we have made every attempt to ensure that the information on our quote is accurate, we cannot be held responsible for mistakes or omissions. Please take a few moments to verify the model #’s, quantities, modifications and/or changes (door hinging, etc.) are correct.